Initializing 3D Engine
Loading OpenCascade...

# Cell Holder Generator

Generate custom 3D printable cell holders with STEP export

Series (S) Cells stacked in series. Sets voltage.
Parallel (P) Cells bundled in parallel. Sets capacity.
Width (mm)
Depth (mm)
Cells are fit automatically inside the footprint.
Holder Thickness (mm)
Cell Diameter (mm)
Layout Type
Cell Spacing (mm)
Ledge Thickness (mm)
Ledge Width (mm)
Rounded Corners
Opening Type
Hole Diameter (mm)
Tab Width (mm)
Tab Depth (mm)
Export Format
STEP exports a 3D solid for CAD or 3D printing. DXF exports a flat 2D outline for laser or plasma cutters.

## Preview

Configure settings and click Generate to see preview