
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "BM05B-GHS-TBT_LF__SN__N_" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -5.08 10.922 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "BM05B-GHS-TBT_LF__SN__N_" (id 1) (at -5.08 -12.7 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "BM05B-GHS-TBT_LF__SN__N_:JST_BM05B-GHS-TBT_LF__SN__N_" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "JST Sales" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "4.05 mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "None" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/BM05B-GHS-TBT(LF)(SN)(N)/JST/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/BM05B-GHS-TBT(LF)(SN)(N)/JST/view-part/?ref=snap" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "BM05B-GHS-TBT(LF)(SN)(N)" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            Connector Header Surface Mount 5 position 0.049 (1.25mm)\n                        \n" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "In Stock" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "JST" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "BM05B-GHS-TBT_LF__SN__N__0_0"
      (polyline
        (pts (xy -3.81 -10.16) (xy -5.08 -8.89)) (stroke (width 0.254))
      )
      (polyline
        (pts (xy -5.08 8.89) (xy -3.81 10.16)) (stroke (width 0.254))
      )
      (polyline
        (pts (xy -5.08 7.62) (xy -3.175 7.62)) (stroke (width 0.254))
      )
      (rectangle (start -4.445 7.3025) (end -2.8575 7.9375)
        (stroke (width 0.1)) (fill (type outline))
      )
      (polyline
        (pts (xy -5.08 5.08) (xy -3.175 5.08)) (stroke (width 0.254))
      )
      (rectangle (start -4.445 4.7625) (end -2.8575 5.3975)
        (stroke (width 0.1)) (fill (type outline))
      )
      (polyline
        (pts (xy -5.08 2.54) (xy -3.175 2.54)) (stroke (width 0.254))
      )
      (rectangle (start -4.445 2.2225) (end -2.8575 2.8575)
        (stroke (width 0.1)) (fill (type outline))
      )
      (polyline
        (pts (xy -5.08 0.0) (xy -3.175 0.0)) (stroke (width 0.254))
      )
      (rectangle (start -4.445 -0.3175) (end -2.8575 0.3175)
        (stroke (width 0.1)) (fill (type outline))
      )
      (polyline
        (pts (xy -5.08 -2.54) (xy -3.175 -2.54)) (stroke (width 0.254))
      )
      (rectangle (start -4.445 -2.8575) (end -2.8575 -2.2225)
        (stroke (width 0.1)) (fill (type outline))
      )
      (rectangle (start -4.64704545455 -10.16) (end 5.51295454545 10.16)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin passive line (at -10.16 7.62 0) (length 5.08)
        (name "1"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -10.16 5.08 0) (length 5.08)
        (name "2"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -10.16 2.54 0) (length 5.08)
        (name "3"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -10.16 0.0 0) (length 5.08)
        (name "4"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -10.16 -2.54 0) (length 5.08)
        (name "5"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -10.16 -7.62 0) (length 5.08)
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "S1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -10.16 -7.62 0) (length 5.08)
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "S2"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)